SECTION 095123 – USG “F” FISSURED™ BASIC ACOUSTICAL TILE CEILINGS

**USG “F” FISSURED™ BASIC**

* Cast product with durable surface that resists scrapes commonly caused by accessing the ceiling plenum.
* Zero VOC emissions exceeds CA Specification 01350.
* High recycled content. USDA Certified Biobased Product
* 12"x12" tile with the USG Donn Brand DX®/DXL™ Concealed Suspension System creates a “gridless” appearance.
* **<Insert product representative here>** or 800.874.4968 for technical questions.

**Note to specifiers:**

This document is not intended to function as a standalone specification. It is intended to assist the specifier in inserting the proper language into the following recommended specification sections:

* 09 51 13 Acoustical Panel Ceilings
* 09 51 23 Acoustical Tile Ceilings

2.3 ACOUSTICAL TILES

* + - * 1. Acoustical Panel Type **<INSERT DESIGNATION HERE>**:

Basis of Design: Subject to compliance with project requirements, the design is based on the following: USG Interiors, LLC, “F Fissured Basic”.

Classification: Provide ceiling panels complying with ASTM E 1264 for type, form and pattern as follows:

Type: III, mineral base with painted finish

Form: 4, Cast or Molded

Pattern: D, Fissured

Color: Flat White 050.

LR: Not less than 0.79.

NRC: Not less than 0.70.

CAC: Not less than **[25] [35].**

Edge/Joint Detail: **[FL Flush reveal] [BESK Beveled, kerfed and rabbeted] [SL Reveal] [SQ Square].**

Suspension Grid/Width: **[DX/DXL] [DXW] [DXT] [DXF] [DXFF] [DXI] [9/16 inch (14 mm)] [15/16 inch (24 mm)] [1 ½ inch (38 mm)].**

Panel Thickness: 3/4 inch (19 mm).

Modular Size: **[12 by 12 inches (305 by 305 mm)] [24 by 24 inches (610 by 610 mm) with foil back] [24 by 48 inches (610 by 1220 mm) with foil back] [As indicated on Drawings] [As indicated in a schedule].**

Recycled Content: 69%

High Recycled Content: Classified as containing greater than 50% total recycled content. Total recycled content is based on product composition of post-consumer and pre-consumer post-industrial recycled content per FTC guidelines.

VOC Emissions: Third party (GREENGUARD Gold) certified for low-emitting performance, meets California Department of Department of Public Health’s (CDPH) Standard Method v1.1-2010 (CA Section 01350). ‘Certificates of Compliance’ for Low VOC Emissions are available on usg.com and at productguide.ulenvironment.com.

Disclaimer: The USG Product Specifications contained herein are intended for use as product reference material by architects, engineers, other design professionals, contractors, building code officials, or other competent construction industry trade professionals having an interest in the selection, specification and use of products manufactured by the subsidiaries of USG Corporation. The Specifications are intended solely as technical support incident to the sale and use of USG products and not intended to be a substitute for the design review and approval of the licensed design professionals for the project. These materials may be printed and/or transferred electronically solely as needed by the user. Because electronic text files can be modified by other parties, without notice or indication of such modifications, modification of USG Product Guide Specifications and Drawings is the sole responsibility of the Design Professional.