SECTION 09 51 23 – USG RADAR™ EDUCATION ACOUSTICAL TILE CEILINGS

**USG RADAR™ EDUCATION**

* ClimaPlus™ 30 year limited system warranty performance
* High-NRC/High-CAC formulation helps to comply with ANSI S12.60 Classroom Guidelines (LEED for schools).
* Excellent Sound Absorption. Available with 40 CAC for increased room to room speech privacy and 0.70 NRC for greater sound control in classrooms.
* Optional Firecode® product designed to meet life safety codes
* USDA Certified Biobased Product
* High Durability panels are 55% more durable than standard panels
* Non directional pattern reduces installation time and waste
* **<insert product representative here>** or 800.874.4968 for technical questions

**Note to specifiers:**

This document is not intended to function as a standalone specification. It is intended to assist the specifier in inserting the proper language into the following recommended specification sections:

* 09 51 13 Acoustical Panel Ceilings
* 09 51 23 Acoustical Tile Ceilings

|  |
| --- |
| **Sustainability Notes:** (Architecture 2030 Challenge for Products - LEED v4 EPD/LCA improvements) |
| * Third party (GREENGUARD Gold) certified for low-emitting performance, meets California Department of Public Health’s (CDPH) Standard Method v1.1-2010 (CA Section 01350). “Certificates of Compliance’ available on usg.com and at productguide.ulenvironment.com.
 |

2.3 ACOUSTICAL TILES

* + - * 1. Acoustical Panel Type **<INSERT DESIGNATION HERE>**:

Basis of Design: Subject to compliance with project requirements, the design is based on the following: USG Interiors, LLC, “Radar Education”.

Classification: Provide ceiling panels complying with ASTM E 1264 for type, form and pattern as follows:

Type: III, mineral base with painted finish

Form: 2, water felted

Pattern: C & E, perforated, small holes and light texture

Color: Flat White 050.

LR: Not less than 0.84.

NRC: Not less than **[0.55] [0.70].**

CAC: Not less than **[35] [40].**

Edge/Joint Detail: **[SLT Beveled Reveal] [FLB Flush reveal] [SQ Square].**

Suspension Grid/Width: **[DX/DXL] [DXT] [DXLT] [DXW] [DXF] [DXFF] [DXI] [DXLF] [9/16 inch (14 mm)] [15/16 inch (24 mm)] [1 ½ inch (38 mm)].**

Panel Thickness: **[5/8 inch (15.9 mm)] [3/4 inch (19 mm)] [7/8 inch (23 mm)].**

Modular Size: **[24 by 24 inches (610 by 610 mm)] [24 by 48 inches (610 by 1220 mm)] [As indicated on Drawings] [As indicated in a schedule].**

Recycled Content: Up to 57%.

VOC Emissions: Third party (GREENGUARD Gold) certified for low-emitting performance, meets California Department of Public Health’s (CDPH) Standard Method v1.1-2010 (CA Section 01350). “Certificates of Compliance’ available on usg.com and at productguide.ulenvironment.com.

Panel Options:

[Firecode®: a Fire rated option, designed to meet life safety codes].

[High Recycled Content: Classified as containing greater than 50% total recycled content. Total recycled content is based on product composition of post-consumer and pre-consumer (post-industrial) recycled content per FTC guidelines.].

[High durability abuse resistant panels].

ClimaPlus™ 30 year limited system warranty performance: Contains a broad spectrum antimicrobial additive on the face and back of the panel that provides resistance against the growth of mold and mildew. Includes sag resistance performance.

Disclaimer: The USG Product Specifications contained herein are intended for use as product reference material by architects, engineers, other design professionals, contractors, building code officials, or other competent construction industry trade professionals having an interest in the selection, specification and use of products manufactured by the subsidiaries of USG Corporation. The Specifications are intended solely as technical support incident to the sale and use of USG products and not intended to be a substitute for the design review and approval of the licensed design professionals for the project. These materials may be printed and/or transferred electronically solely as needed by the user. Because electronic text files can be modified by other parties, without notice or indication of such modifications, modification of USG Product Guide Specifications and Drawings is the sole responsibility of the Design Professional.