111R12.240
Fire door fitting with split spindle
in R-technology with roses according to DIN 18255 and EN 1906 made of polyamide, high-polished surface, consisting of: 
Lever handle model 111.23R U-shaped made of high-quality polyamide with corrosion resistant steel insert, solid colour, diameter 23 mm, with stepped shoulder guide and groove, easily installed by latching the lever handle into the base parts pre-mounted on the door. 
The latching can be released using the dismantling tool. The lever handle meets the standards of EN 179 and DIN 18040.
Roses: model 315.23... and 316RFS roses substructure made of synthetic material-stainless steel composite, can be used for left and right-hand opening doors. Fixed rotating bearing of the lever handle with automatically latching all-round locking and 5 mm journal as maintenance-free plain bearing with elastic compensating area and second journal in the neck of the lever handle. Concealed, non-loosening screwed joint. 
Rose cap, oval, made of polyamide, solid colour, 31 x 72 mm, 10.5 mm high, flat, 1.5 mm wall thickness.
Designed and tested for the projects segment, user category to EN 1906 - Class 4 fire door fitting with spindle 9 mm, according to DIN 18273
user category: Class 4
Durability: Class 7
Door weight: No classification specified
Fire resistance: Class D1
Safety: Class 1
Corrosion resistance: Class 4
Burglary protection: Class 0
Design-type: U

Article no.: HEWI 111R12.240

